|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Monthly Overview** | | | **May 16th, 2022 – June 20th, 2022** | | | | |  | |
| * **Fixed a severe washout on 170th-6 Hauled dirt from Borrow pit on 180th-06** * **Repaired washouts from heavy rains** * **R & R ac compressor on pt-2** * **R&R CB radio in pt2** * **Replaced last 4 tires on belly dump** * **R&R Brake pods on belly dump** * **Graded Roads (See Below)** * **Rocked several road** * **Charged ac on roller** * **Installed several culverts** * **County hauled us several loads of dirt.** * **Stripped topsoil off borrow pit on 180th-6** * **Stripped Topsoil off borrow pit on Countyline-3** * **Started hauling material to build up CL-3**   **Next Months plan of work**   * **Fix Water Truck** * **Finish Repairs from rain damage** * **Repair chip seal roads** * **Continue building up chipseal roads**   **Totals for the Month** | | | | | | |  | |
|  | | | | | | |  | |
| Materials hauled by Township | +/- | Ton Rock | | Fuel Dispensed - Unleaded Gas |  | Gallons | |  | |
| Materials hauled by Contractors | +/- | Ton Rock | | Fuel Dispensed - Red Diesel |  | Gallons | |  | |
| Dirt Hauled by Both | 63 | Loads | | Fuel Dispensed - Green Diesel |  | Gallons | |  | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Equipment Status** | | | | | |
| **Unit** | **Usable** | **Notes** | **Unit** | **Usable** | **Notes** |
| Cat 160M3 Grader | Yes |  | Sterling Dump Truck (PT-3) | Yes |  |
| Cat Backhoe | Yes |  | Ford F-250 (PT-4) | Yes | vacuum pump |
| John Deere 4816 Mower | Yes | Instrument panel inop | Freightliner M2 (PT-5) | Yes | Tank,brakeandturnlights |
| John Deere 135G Excavator | Yes |  | Hamm Roller 3412 | Yes |  |
| International DuraStar (PT-1) | Yes | Turn signal ghost | Diamond Mower | Yes | Drive shaft |
| International ProStar (PT-2) | yes | Air tank bracket broke/air pod leaking | John Doere HX-15 Mower | Yes |  |

**Graded Roads** – All roads were graded at least once